ETS-1 Maritime
Monitoring Plan Checklist

To be used by shipping companies and verifiers to ensure that Monitoring Plans (MPs) meet minimum quality requirements for a subsequent assessment and approval by the Administering Authority (AA). 
If the submitted MP does not meet the criteria listed below, it will be returned to the shipping company for further improvements.

	
	Topic
	Requirement

	☐

	Docs
	Documents required by AA are uploaded to THETIS-MRV which includes at minimum:
· Risk Assessment
· Verifier’s Statement
· Mandate (only applicable in the case of ISM company - application date 01.01.2024 or earlier)  – if the mandate has been signed later in 2024, an explanation should be provided (e.g. change of the ship’s owner)

	☐	Description of procedures
	Check all tabs and sub-tabs in THETIS-MRV MP and make sure that you added descriptions of ALL relevant procedures. Please note that mere references to existing documents and procedures are not sufficient!
For ICE class vessels, it is recommended to describe additional procedures applicable only to ICE class vessel under the tab “Navigation” - “voluntary monitoring” provision as outlined in Annex 1 Part C.6 of the Commission Implementing Regulation 2023/2449

	☐	Data alignment across tabs 
	1. Measuring Equipment – Monitoring Methods: Measuring equipment shall correspond to the monitoring methods listed in the tabs “Emission sources” and “Fuel tanks” as well as in the sub-tab “Data gaps” under “Fuel consumption”. 
Example: If only gauge tapes are listed as measuring equipment, the shipping company cannot use Method C “Flow meters” as either main or back-up monitoring method!

2. Emission Sources – Fuel Tanks – Fuel Types and EF: The list of fuels shall be one and the same for all tabs. Fuels listed under “Fuel types and EF” should be linked to the respective emission sources and fuel tanks. 
Example: If HFO, LFO, MDO and MDG are listed in the tabs “Emission sources” and “Fuel tanks”, only HFO, LFO, MDO and MDG shall be listed in the tab “Fuel types and EF”

	☐	Emission Sources
	List all emission sources, including waste incinerator, auxiliary engines, inert gas generator, etc.

	☐	Fuel Tanks
	List each fuel tank separately! Entries such as “All fuels” or “All tanks” will not be accepted.

	☐	Level of Uncertainty
	Ensure that level of uncertainty is either 10% or 7.5%. Any other “ship-specific” value may be accepted upon the submission of the respective uncertainty assessment.
A separate guidance document on the assessment of uncertainty in the EU ETS for stationary installations is provided (GD No. 492).



